UNITE 180: Install PanoCAM Studio NOOTA


Device list: Windows 10 PC, USB Type-A to Type-C cable, UNITE 180 Camera


1. Connect the UNITE 180 camera to the PC. When detected, Windows will open file explorer to the CD Drive. Below you will notice that Windows has assigned drive F.

Graphical user interface, application, Word

Description automatically generated

NOTE: If Windows assigns the CD Drive another drive letter, you will need to edit the copy\_studio.bat file, located in the Studio Update folder, accordingly.





1. Launch copy\_studio.bat. Wait for studio replacement to complete (about 60s). The camera will restart after the copy is complete. Verify PanoCAMStudioSetup\_v2317\_NOOTA.exe and PanoCAMStudioSetup\_v2401\_NOOTA.pkg are present in the CD Drive.

